|  |
| --- |
| If control measures aren’t implemented and effectiveit is rated **HIGH RISK** (50 ): Severity(10 ) x Likelihood(5 ) |

|  |  |  |
| --- | --- | --- |
| Groups at risk • engineers / maintenance • Lone workers• Contractors• Club members | Hazards • Slips, trips and falls• Falls from height• Manual handling injury | Practices resulting in hazards • Maintenance work above head height or on roof. |

|  |
| --- |
| Control Measures • Work at height assessment prior to work commencing.• Safe working procedures implemented.• Contractor permit to work system in place.• Routine periodic safety checks on those working at height.• Avoidance of lone working.• Safety signs in place.• Maintenance of ladders and equipment.• Follow safe ladder use procedures.• Ensure three points of contact when using ladders.• Use of alternative lifting measures for carrying items vertical distances if ladder safetyIs compromised.• Safer practice of working in pairs. |

|  |
| --- |
| **After Control Measures:** Severity(10 ) x Likelihood(2 )MEDIUM RISK(20 ) |

Responsible Person: T P Aston. Responsible Person Signature: Tim Aston

Date 03 December 2021 – To be reviewed annually.

Review Date:

|  |  |  |
| --- | --- | --- |
| 08 Nov 22 - TA |  |  |
|  |  |  |
|  |  |  |
|  |  |  |